[READme.txt for Dayton-Hara satellite image.]


The enclosed pair of files is a high-resolution 1-mile-square image of the area surrounding the Dayton Hamvention area in Trotwood Ohio in .BMP format, along with the .SAT calibration file required to use it in UIview.   

This image can be used as a underlay with the Precision Mapping Server Ver 7.07 or Ver 9 for UIview.  Copy to the \Underlays folder located below the main install folder for PMapServer7 or PMapServer9.   Then use the PMap Server control panel in UIview to select "Underlay, Load Underlay" to place this image underneath the Precision Mapping road layer.    
Note that you MUST have Precision Mapping 7, 8 or 9, and the matching PMap Server running in your UIview installation to use this underlay.  It WILL NOT work with static maps.